{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["能效领跑者"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"能效领跑者","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"merged":[[1,0,1,6],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[4,0,4,6],[5,6,8,6],[9,0,9,6],[11,0,11,6],[12,0,13,0],[12,6,13,6],[14,0,14,6],[15,0,18,0],[15,6,18,6],[21,0,21,6],[22,0,23,0],[22,6,24,6],[25,0,25,6],[26,0,30,0],[33,0,38,0],[39,0,40,0],[39,6,40,6],[41,0,41,6],[42,6,44,6],[45,0,45,6],[46,0,47,0],[46,6,48,6]],"flags":["formulas_cached_only"]}
["附件1"]
["2024年广东省重点行业“能效领跑者”名单"]
["能效“领跑者”企业名称","主要能效指标","实际值","单位","国内先进值","能耗限额标准先进值","备注"]
[]
["纺织行业"]
["佛山市顺德金纺集团有限公司","棉针织染整布单位产品综合能耗",553.16," kgce/t",1000,"≤1300","T/GDTEX 27-2022        《广东省机织染整布和针织染整布单位产品综合能耗限额》"]
["佛山市南海雄科纺织有限公司","棉机织坯布单位产品综合能耗",3.01," kgce/t","▬","▬"]
["佛山市亚纺染整有限公司","棉机织染整布单位产品综合能耗",10.98," kgce/hm",35,"≤68"]
["广东前进牛仔布有限公司","牛仔色纱单位产品综合能耗",10.23," kgce/hm",25,"▬"]
["水泥行业"]
["广东清远广英水泥有限公司","熟料单位产品综合能耗",95.56," kgce/t",100,100,"GB16780-2021 水泥单位产品能源消耗限额"]
["钢铁行业"]
["宝钢湛江钢铁有限公司","烧结工序",38.84," kgce/t",{"v":39.9,"d":"39.90"},45,"GB21256-2013粗钢生产主要工序单位产品能源消耗限额"]
[null,"转炉工序",-32.24," kgce/t",-32.06,-30]
["有色金属行业"]
["佛山市三水凤铝铝业有限公司","圆铸锭",115.09," kgce/t","▬",120,"GB 21351-2014铝建筑型材单位产品能源消耗限额"]
[null,"基材",99.02," kgce/t","▬",120]
[null,"氧化电泳型材",104.32," kgce/t","▬",140]
[null,"喷涂型材",43.19," kgce/t","▬",60]
["广州铜材厂有限公司","铜板带材",193.11," kgce/t","▬",370,"GB 29442-2012铜板带箔材单位产品能源消耗限额"]
["佛山市华鸿铜管有限公司","铜管材",{"v":111.9,"d":"111.90"}," kgce/t","▬",450,"GB 21350-2013铜管材单位产品能源消耗限额"]
["造纸行业"]
["山鹰纸业（广东）有限公司","箱纸板",175.38," kgce/t","▬",290,"GB31825-2015 制浆造纸单位产品能源消耗限额"]
[null,"瓦楞原纸",171.41," kgce/t","▬",270]
["江门中顺纸业有限公司","生活用纸",{"v":255.7,"d":"255.70"}," kgce/t","▬",420]
["石油化工行业"]
["中国石油化工股份有限公司广州分公司","原油加工",6.54,"千克标油/吨·因数",6.02,{"v":7,"d":"7.0"},"GB 30251-2013 炼油单位产品能源消耗限额"]
[null,"低压聚乙烯",92.06,"千克标油/吨","▬","▬","DB44/ 1297-2014聚乙烯单位产品能源消耗限额"]
[null,"延迟焦化2#",19.94,"千克标油/吨","▬","▬","▬"]
[null,"MTBE2＃",80.91,"千克标油/吨","▬","▬","▬"]
[null,"干气制苯乙烯",417.83,"千克标油/吨","▬",435,"GB 32053-2015苯乙烯单位产品能源消耗限额"]
["中国石油化工股份有限公司茂名分公司","渣油加氢（固定床）",10.18,"千克标油/吨","▬","▬","▬"]
["中海壳牌石油化工有限公司","高压聚乙烯",138.87,"千克标油/吨","▬","▬","DB44/ 1297-2014聚乙烯单位产品能源消耗限额"]
["中科（广东）炼化有限公司","常减压蒸馏",6.05,"千克标油/吨","▬","▬","▬"]
[null,"催化裂化",36.24,"千克标油/吨","▬","▬","▬"]
[null,"加氢裂化",12.74,"千克标油/吨","▬","▬","▬"]
[null,"连续重整",43.71,"千克标油/吨","▬","▬","▬"]
[null,"柴油加氢",3.79,"千克标油/吨","▬","▬","▬"]
[null,"聚丙烯1＃",53.64,"千克标油/吨","▬","连续气相法：48，连续液相本体法：51","GB 31826- 2015聚丙烯单位产品能源消耗限额"]
["广东石化有限责任公司","乙烯裂解（单位乙烯能耗）",569.95,"千克标油/吨",513,610,"GB 30250-2013 乙烯装置单位产品能源消耗限额"]
[null,"乙烯裂解（单位双烯能耗）",389.08,"千克标油/吨","▬",400]
["玻璃行业"]
["东莞南玻太阳能玻璃有限公司（500吨/天浮法玻璃生产线）","单位产品综合能耗（800吨/天以下平板玻璃生产线，含800吨/天）",8.93,"kgce/重量箱",8.92,9.5,"《玻璃和铸石单位产品能源消耗限额》（GB21340-2019）"]
["信义超薄玻璃（东莞）有限公司（F线900吨/天平板玻璃生产线）","单位产品综合能耗（800吨/天以上平板玻璃生产线）",9,"kgce/重量箱","▬",8]
["肇庆南玻节能玻璃有限公司","单位产品综合能耗（6mm平面普通钢化玻璃）",3.49,"kw·h/m2","▬",3.22]
["陶瓷行业"]
["广东清远蒙娜丽莎建陶有限公司","E≤0.5%的陶瓷砖",3.85,"kgce/㎡",{"v":2.8,"d":"2.80"},{"v":4,"d":"4.00"},"工业重点领域能效标杆水平和基准水平（2023年版）"]
[null,"0.5%＜吸水率E≤10%的陶瓷砖",3.01,"kgce/㎡","▬",{"v":3.7,"d":"3.70"}]
["佛山市高明安华陶瓷洁具有限公司","卫生陶瓷",252.8,"kgce/t",282.28,300]
["注：相关数据基准年度为2023年度，符号“▬”表示国家暂无遴选相关工序的“领跑者”，或暂无相关工序的能耗限额标准。                    "]